
These programs are designed for JK Microsystem's uFlash embedded
processor with it's matching A/D and temperature probes.

THERM.EXE
    The example demonstrates:
    - basic interfacing with the A/D board
    - integer temperature calcuations in both Fahrenheit and Celcius degrees
    - fixed point decimal calculations in both Fahrenheit and Celcius degrees

    Note, the uFlash board does not have a math co-processor (80387), and
    Borland's floating point emulation libaries are not compatible with
    pre-emptive threading.  So this example uses eRTOS's fixed point
    eMATH functions when accuracy is needed.


TSCOPE.EXE
    (TSCOPE.C, WEBPART.C)
    This example builds on THERM to create a web server which doles up
    Dynamic HTML with the current temperature, and presents a graph of
    recent temperature readings.

    For this example, all calculations are done in integer math.

Note:
  The LDRIVER.* files are slightly reworked versions of JK Micro's DRIVER.*
  files.  However, DRIVER.ASM was hard coded for small model, so LDRIVER.ASM
  is adjusted to use large model stacks and large model parameter passing.


